# 2.8inch RPi LCD (A)

### Description:

This is a 2.8inch TFT LCD with resistive touch panel, has 320x240 resolution. It can support any revision of Raspberry Pi. Driver is provided for Raspbian/Ubuntu Mate/kali.

### Website：

CN: http://www.waveshare.net/shop/2.8inch-RPi-LCD-A.htm

EN: https://www.waveshare.com/2.8inch-rpi-lcd-a.htm

### WIKI：

CN: http://www.waveshare.net/wiki/2.8inch_RPi_LCD_(A)

EN: https://www.waveshare.com/wiki/2.8inch_RPi_LCD_(A)

### Driver install：

sudo ./LCD28-show


# 3.2inch RPi LCD (B)

### Description:

This is a 3.2inch TFT LCD with resistive touch panel, has 320x240 resolution. Can support any revision of Raspberry Pi. Driver is provided for Raspbian/Ubuntu Mate/kali. 

### Website：

CN: http://www.waveshare.net/shop/3.2inch-RPi-LCD-B.htm

EN: https://www.waveshare.com/3.2inch-rpi-lcd-b.htm

### WIKI：

CN: http://www.waveshare.net/wiki/3.2inch_RPi_LCD_(B)

EN: https://www.waveshare.com/wiki/3.2inch_RPi_LCD_(B)

### Driver install:

sudo ./LCD32-show

# 3.2inch RPi LCD (C)

### Description: 

This is a 3.2inch TFT LCD with resistive touch panel, has 320x240 hardware resolution.Support up to 125MHz high-speed SPI signal transmission provide you a clear and stable display effect.. Can directly plug to any revision of Raspberry Pi. Driver is provided for Raspbian/Ubuntu Mate/kali and Retropie(Can only display when working with Retropie).

### Website:

CN: http://www.waveshare.net/shop/3.2inch-RPi-LCD-C.htm

EN: https://www.waveshare.com/3.2inch-rpi-lcd-c.htm

### WIKI:

CN: http://www.waveshare.net/wiki/3.2inch_RPi_LCD_(C)

EN: https://www.waveshare.com/wiki/3.2inch_RPi_LCD_(C)

### Driver install:

sudo ./LC32C-show

# 3.5inch RPi LCD (A)

### Description:

This is a 3.5inch TFT LCD with resistive touch panel, has 480x320 resolution. Can support any revision of Raspberry Pi. Driver is provided for Raspbian/Ubuntu Mate/kali. 

### Website:

CN:http://www.waveshare.net/shop/3.5inch-RPi-LCD-A.htm

EN:https://www.waveshare.com/product/3.5inch-rpi-lcd-a.htm

### WIKI:

CN:http://www.waveshare.net/wiki/3.5inch_RPi_LCD_(A)

EN:https://www.waveshare.com/wiki/3.5inch_RPi_LCD_(A)

### Driver install:

sudo ./LCD35-show

# 3.5inch RPi LCD (B)

### Description:

This is a 3.5inch TFT LCD with resistive touch panel, has 480x320 resolution. Can support any revision of Raspberry Pi. Driver is provided for Raspbian/Ubuntu Mate/kali. And this is an IPS screen which has wider viewing angle.

### Website:

CN:http://www.waveshare.net/shop/3.5inch-RPi-LCD-B.htm

EN:https://www.waveshare.com/3.5inch-RPi-LCD-B.htm

### WIKI:

CN:http://www.waveshare.net/wiki/3.5inch_RPi_LCD_(B)

EN:https://www.waveshare.com/wiki/3.2inch_RPi_LCD_(B)

### Driver install:

sudo ./LCD35B-show V2

# 3.5inch RPi LCD (C)

### Description:

This is a 3.5inch TFT LCD with resistive touch panel, has 480x320 resolution. Support up to 125MHz high-speed SPI signal transmission provide you a clear and stable display effect.. Can directly plug to any revision of Raspberry Pi. Driver is provided for Raspbian/Ubuntu Mate/kali and Retropie(Can only display when working with Retropie).

### Webiste：

CN:http://www.waveshare.net/shop/3.5inch-RPi-LCD-C.htm

EN:https://www.waveshare.com/3.5inch-rpi-lcd-c.htm

### WIKI：

CN:http://www.waveshare.net/wiki/3.5inch_RPi_LCD_(C)

EN:https://www.waveshare.com/wiki/3.5inch_RPi_LCD_(C)

### Driver Install：

sudo ./LCD35C-show

# 3.5inch HDMI LCD

### Description:

This is a 3.5inch IPS screen with resistive touch panel, has 480x320 hardware resolution, use HDMI interface for displaying and GPIO for touching. Touch driver is provide for Raspbian, Ubuntu Mate,Kali and Retropie(Can only display when working with Retropie).

### Website:

CN: http://www.waveshare.net/shop/3.5inch-HDMI-LCD.htm

EN: https://www.waveshare.com/product/3.5inch-hdmi-lcd.htm

### WIKI:

CN: http://www.waveshare.net/wiki/3.5inch_HDMI_LCD

EN: https://www.waveshare.com/wiki/3.5inch_HDMI_LCD

### Display setting:

For properly display, you need to root directory of SD card (/boot/).

max_usb_current=1

hdmi_group=2

hdmi_mode=87

hdmi_cvt 800 480 60 6 0 0 0

hdmi_drive=2

### Driver install (touch):

sudo ./LCD35-HDMI-480x320-show

# 4inch RPi LCD (A)

### Description:

This is a 4inch resistive LCD, IPS screen, 480x320 resoltuion, designed for Raspberry Pi. Driver is required for Raspbian, Ubuntu Mate,Kali.

### Website:

CN: http://www.waveshare.net/shop/4inch-RPi-LCD-A.htm

EN: https://www.waveshare.com/4inch-RPi-LCD-A.htm

### Wiki:

CN: http://www.waveshare.net/wiki/4inch_RPi_LCD_(A)

EN: https://www.waveshare.com/wiki/4inch_RPi_LCD_(A)

### Driver install:

sudo ./LCD4-show

# 4inch RPi LCD (C)

### Description:

This is a 4inch TFT LCD with resistive touch panel, has 480x320 resolution. Support up to 125MHz high-speed SPI signal transmission provide you a clear and stable display effect. Can directly plug to any revision of Raspberry Pi. Driver is provided for Raspbian/Ubuntu Mate/kali and Retropie(Can only display when working with Retropie).

### Website:

CN: http://www.waveshare.net/shop/4inch-RPi-LCD-C.htm

EN: https://www.waveshare.com/4inch-rpi-lcd-c.htm

### WiKi:

CN: http://www.waveshare.net/wiki/4inch_RPi_LCD_(C)

EN: https://www.waveshare.com/wiki/4inch_RPi_LCD_(C)

### Driver install:

sudo ./LCD4C-show

# 4inch HDMI LCD 

### Description:

This is a 4inch IPS screens, 800x480 resolution, HDMI display. Designed for Raspberry Pi. Note that this screen is vertically display by default.

### Website:

CN: http://www.waveshare.net/shop/4inch-HDMI-LCD.htm 

EN: https://www.waveshare.com/4inch-hdmi-lcd.htm

### WiKi:

CN: http://www.waveshare.net/wiki/4inch_HDMI_LCD

EN: https://www.waveshare.com/wiki/4inch_HDMI_LCD

### Display Setting:

hdmi_group=2

hdmi_mode=87

hdmi_cvt 480 800 60 6 0 0 0

dtoverlay=ads7846,cs=1,penirq=25,penirq_pull=2,speed=50000,keep_vref_on=0,swapxy=0,pmax=255,xohms=150,xmin=200,xmax=3900,ymin=200,ymax=3900

display_rotate=3

### Driver Install:

sudo ./LCD4-800x480-show

# 4.3inch HDMI LCD 

### Description:

This is a 4.3inch IPS screens, 800x480 resolution, HDMI display. Designed for Raspberry Pi. Driver is required for touching. Note that this LCD can only support Raspberry Pi

### Website:

CN: http://www.waveshare.net/shop/4.3inch-HDMI-LCD.htm

EN: https://www.waveshare.com/wiki/4inch_HDMI_LCD

### WiKi:

CN: http://www.waveshare.net/wiki/4.3inch_HDMI_LCD

EN: https://www.waveshare.com/wiki/4.3inch_HDMI_LCD

### Display Setting:

display_rotate=2

max_usb_current=1

hdmi_group=2

hdmi_mode=87

hdmi_cvt 480 272 60 6 0 0 0

dtoverlay=ads7846,cs=1,penirq=25,penirq_pull=2,speed=50000,keep_vref_on=0,swapxy=0,pmax=255,xohms=150,xmin=200,xmax=3900,ymin=200,ymax=3900

hdmi_drive=1

hdmi_force_hotplug=1

### Driver Install:

sudo ./LCD43-show-V2

# 5inch HDMI LCD

### Description:

This is a 5inch Resistive Touch Screen LCD, 800x480 resolution, HDMI interface. Designed for Raspberry Pi. Note that this LCD can only support Raspberry Pi.

### Website:

CN: http://www.waveshare.net/shop/5inch-HDMI-LCD.htm

EN: https://www.waveshare.com/product/5inch-hdmi-lcd.htm

### WiKi:

CN: http://www.waveshare.net/wiki/5inch_HDMI_LCD

EN: https://www.waveshare.com/wiki/5inch_HDMI_LCD

### Display Setting:

max_usb_current=1

hdmi_group=2

hdmi_mode=87

hdmi_cvt 800 480 60 6 0 0 0

hdmi_drive=1

### Driver Install:

sudo ./LCD5-show

# 7inch HDMI LCD

### Description:

This is a 7inch resistive touch screen LCD, 1024x600 resolution, HDMI interface, designed for Raspberry Pi

### Website:

CN:http://www.waveshare.net/shop/7inch-HDMI-LCD.htm

EN:https://www.waveshare.com/product/7inch-hdmi-lcd.htm

### WiKi:

CN:http://www.waveshare.net/wiki/7inch_HDMI_LCD

EN:https://www.waveshare.com/wiki/7inch_HDMI_LCD

### Display Setting:

max_usb_current=1

hdmi_group=2

hdmi_mode=87

hdmi_cvt 1024 600 60 6 0 0 0

### Driver install:

sudo ./LCD7-1024x600-show

# 10.1inch HDMI LCD
### Description

This is a 10.1inch resistive touch screen LCD, 1024x600 resolution, HDMI interface, designed for Raspberry Pi

### Website:

CN:http://www.waveshare.net/shop/10.1inch-HDMI-LCD.htm

EN:https://www.waveshare.com/product/10.1inch-hdmi-lcd.htm

### WiKi:

CN:http://www.waveshare.net/wiki/10.1inch_HDMI_LCD

EN:https://www.waveshare.com/wiki/10.1inch_HDMI_LCD

### Display Setting:

max_usb_current=1

hdmi_group=2

hdmi_mode=87

hdmi_cvt 1024 600 60 6 0 0 0

### Driver install:

sudo ./LCD101-1024x600-show
